**602 Crate Late Model Sportsman**
HTS 1350, HTS 1600, Crate 21 or Crate 55, American Racer 48 & 56. Samples will be taken - Grooving and siping are allowed.

Any 4 Barrel Carburetor

Shocks: Nesmith & Thunder Series shock packages. A single bump stop is allowed. No spring rubbers.

One shock per corner, except left rear. May run a drive shock.

Weight 2400 lbs. One pound per lap burn off in Feature. All other times must weigh 2400 lbs.

All spoilers are 8" and 8" sides. Deck is 39" no tolerance.